Logo

Description automatically generated

**RPM-LCD Series**

**Firmware Installation Guide**

**Please read the entire instruction sheet before attempting to update the RPM-LCD firmware.**

1. From a standard web browser, log in to the RPM-LCD unit to be updated. Once logged into the unit, go to **Configuration/System** webpage:

**1**

**NOTE:** For new installations, the default IP-address for the RPM is: **192.168.0.216.** The default Username is **snmp** and the default Password is **1234**.

A screenshot of a computer

AI-generated content may be incorrect.

2. Go to the “Firmware Upgrade” section. Select the “Choose File” button and select the filename of the new firmware to upload.

A screenshot of a computer

AI-generated content may be incorrect.

1. Once the new firmware file is selected, the filename will appear next to the “Choose File” button. Press the Upload button. When the file upload I completed a message will appear that says: “Upload Complete”.

A screenshot of a computer

AI-generated content may be incorrect.

**PDU.fm**

1. When the upload is finished, press the “Update” or “Update and Reset” button.

A screenshot of a computer

AI-generated content may be incorrect.

1. After about 1 minute, refresh the webpage to confirm the update was successful. If the new firmware does not load properly, repeat the process.

Para Systems, Inc / Minuteman Power Technologies

2850 Lake Vista Drive, Suite #110

Lewisville, TX 75067

800.238.7272 / 972.446.7363

minutemanups.com / SizeMyUPS.com

RevA 20251205